| It is easy to upgrade a Scorer with new firmware: i. Select Install in the table unit´s admin menu. ii. Connect the Scorer with the USB cable that belongs to the Base station. iii. Click Programs/BOS package/Run BridgeScorer Firmware upgrade in Windows Start menu. iv. Select Browse in the dialog that appears v. Click Start when you have located the new Scorer firmware vi. WAIT FOR THE INSTALLATION TO BE COMPLETED before disconnecting the USB cable See the manual´s headline F irmware Upgrade for a more detailed description. |  |  |

|  |  | Index |